Lecture Notes - Microwaves

Scribd
Upload a Document
Search Documents

- Sign Up
- |
- Log In

1
First Page
Previous Page
Next Page
/ 18
Sections not available
Zoom Out
Zoom In
Fullscreen
Exit Fullscreen
Select View Mode

#### View Mode

SlideshowScroll
Readcast
Add a Comment
Embed & Share
Reading should be social! Post a message on your social networks to let others know what you're reading. Select the sites below and start sharing.
Readcast this Document

### Login to Add a Comment

### Share & Embed

Add to Collections
Download this Document for Free
Auto-hide: on
Microwaves - Lecture Notes - v.1.3.4 Dr. Serkan Aksoy - 2009
These lecture notes are heavily based on the book of
Microwave Engineering
by David M. Pozar. For future versions or any proposals, please contact with
Dr. Serkan Aksoy
(saksoy@gyte.edu.tr).
Microwaves
Lecture Notes
Dr. Serkan Aksoy
v.1.3.4
2009
Microwaves - Lecture Notes - v.1.3.4 Dr. Serkan Aksoy
–
2009
These lecture notes are heavily based on the book of
Microwave Engineering
by David M. Pozar. For future versions or any proposals, please contact with
Dr. Serkan Aksoy
(saksoy@gyte.edu.tr).
Content
1. LUMPED CIRCUIT MODEL -----------------------------------------1
2. FIELD ANALYSIS of LINES -----------------------------------------1
2.1. Wave Propagation along the Line --------------------------------------------------------------------- 1
2.1.1.
Lossless Transmission Lines ------------------------------------------------------------------------------ 2
2.1.2.
Lossy Transmission Lines --------------------------------------------------------------------------------- 3
2.2. Smith Chart -------------------------------------------------------------------------------------------------- 3
2.3. Slotted Line -------------------------------------------------------------------------------------------------- 4
2.4. Generator & Load Mismatches ------------------------------------------------------------------------- 4
3. MICROWAVE NETWORKS -----------------------------------------5
3.1.
Voltage, Current and Impedance ---------------------------------------------------------------------- 5
3.2. Impedance & Admittance Matrices ------------------------------------------------------------------- 5
3.2.1.
Scattering Matrix -------------------------------------------------------------------------------------------- 5
3.2.2.
Transmission (ABCD) Matrix ---------------------------------------------------------------------------- 6
3.3. Equivalent Circuits for 2 Port Networks ------------------------------------------------------------- 6
3.4. Signal Flow Graphs --------------------------------------------------------------------------------------- 6
4. IMPEDANCE MATCHING ------------------------------------------8
4.1. L Networks Matching ------------------------------------------------------------------------------------- 8
4.2. Quarter Wave Transformer ------------------------------------------------------------------------------ 8
4.3. Single Stub Tuning---------------------------------------------------------------------------------------- 8
4.4. Double Stub Tuning -------------------------------------------------------------------------------------- 9
4.5. Tapered Lines ----------------------------------------------------------------------------------------------- 9
5. POWER DIVIDERS & COUPLERS ------------------------------ 10
5.1. Three Port Networks (T Junction) -------------------------------------------------------------------- 10
5.1.1.
T Junction Power Divider ------------------------------------------------------------------------------- 10
5.2. Four Port Networks (Directional Coupler) --------------------------------------------------------- 10
5.2.1.
Waveguide Directional Coupler ----------------------------------------------------------------------- 10
5.2.2.
Wilkinson Power Divider ------------------------------------------------------------------------------- 11
5.2.3.
Hybrid Coupler -------------------------------------------------------------------------------------------- 11
5.2.4.
Hybrid ------------------------------------------------------------------------------------------------ 11
5.2.5.
Coupled Line Directional Coupler -------------------------------------------------------------------- 11
5.2.6.
Lange Coupler --------------------------------------------------------------------------------------------- 11
5.3. Other Couplers -------------------------------------------------------------------------------------------- 11
6. NOISE & ACTIVE COMPONENTS ----------------------------- 12
6.1. Noise Figure, -------------------------------------------------------------------------------------------- 12
6.2. Dynamic Range & Intermodulation Distortion--------------------------------------------------- 13
6.3. RF Diode Characteristics -------------------------------------------------------------------------------- 14
7. MICROWAVE AMPLIFIER DESIGN --------------------------- 15
7.1. Two-Port Power Gains ---------------------------------------------------------------------------------- 15
7.2. Stability ----------------------------------------------------------------------------------------------------- 15
7.3. Single Stage Amplifier Design ------------------------------------------------------------------------ 16
7.4. Broadband Amplifier Design-------------------------------------------------------------------------- 16
7.5. Power Amplifiers ----------------------------------------------------------------------------------------- 16
7.5.1.
Large Signal Characterization -------------------------------------------------------------------------- 16
Microwaves - Lecture Notes - v.1.3.4 Dr. Serkan Aksoy
–
2009
2 These lecture notes are heavily based on the book of
Microwave Engineering
by David M. Pozar. For future versions or any proposals, please contact with
Dr. Serkan Aksoy
(saksoy@gyte.edu.tr).
2.1.1.
Lossless Transmission Lines
When the lossless line is terminated by a load Reflected waves occur. Reflection coefficient at the load, where and consists of a superposition of an incident and reflected waves called
Standing Waves
().
Time Average Power Flow:
This shows is constant at anywhere on the line.
When the line is matched
  
is constant.
When the line is mismatched (
 
Return Loss
Matched load (No reflected power, maximum power is delivered). Total reflection, (All power reflected). is not constant. The maximum value occurs when. The minimum value occurs when . When increases, increases as a measure of mismatch. Then Standing Wave Ratio() is when means matched line. In that case at , the reflection coefficient and input impedance Using the definition of , more useful form known as
Transmission Line Impedance Equation
as
- Transmission Coefficient:Some part of EM wave is also transmitted to second region as
Insertion Loss
:
Short Circuit: Open Circuit:
The proper length of open or short circuited transmission line can provide any desired reactance or susceptance.
(No regard to ): The same impedance is observed at the input.
(Quarter Wave Transform)- (Short circuit) Open circuit- (Open circuit)
 
Short circuit
Microwaves - Lecture Notes - v.1.3.4 Dr. Serkan Aksoy
–
2009
3 These lecture notes are heavily based on the book of
Microwave Engineering
by David M. Pozar. For future versions or any proposals, please contact with
Dr. Serkan Aksoy
(saksoy@gyte.edu.tr).
2.1.2.
Lossy Transmission Lines
In practice, finite conductivity (or lossy dielectrics) lines can be evaluated as a
Lossy Line
. Low-loss line , . Then ignoring the last term of
  
In the lossy line; , & can be approximated to lossless line.
Distortionless Line
: For the lossy line, in fact the exact is not a linear function of frequency means dispersive. But specifically if the following condition holds then , mean that the lossy line behaves as lossless (distortionless) line.
Terminated Lossy Line
: Loss is assumed small that
Power lost in the line:
Perturbation Method for Calculating Attenuation
Power flow along lossy line: Power loss per unit length: Attenuation constant:
Wheeler Incremental Inductance Rule:
: Incremental inductance: Loss per unit length: Power at the . Then, Attenuation constant: where is skin depth and .
Taylor series Inductance Rule:
where .
2.2.
Smith Chart
where is Resistance, is Reactance, is Conductance and is Susceptance. Whenever is normalized impedance The apsis and ordinate of Smith chart are and . Rearranging them
Microwaves - Lecture Notes - v.1.3.4 Dr. Serkan Aksoy
–
2009
4 These lecture notes are heavily based on the book of
Microwave Engineering
by David M. Pozar. For future versions or any proposals, please contact with
Dr. Serkan Aksoy
(saksoy@gyte.edu.tr).
These are two families of circles as and . Superposition of Smith Chart and its 180
o
() rotated version is known as
Combined Impedance-Admittance Smith Chart
. is the complete revolution of Smith chart. is the half of Smith chart (180
o
). The images of is in Smith chart.
2.3.
Slotted Line
This device is used to find as first .- Measurement of on the distance from the line.- Calculate-- Using and , write- Calculate at .
2.4.
Generator & Load Mismatches
Then, using this where and . where and . Generally is fixed and three cases are considered as
Load Matched to Line: , , . Then . Generator Matched to Line: , . Conjugate Latching:
Maximum power transfer . If one directly chose , it does not mean that the best efficiency due to the phase differences. The efficiency can be improved only by making as small as possible.
Microwaves - Lecture Notes - v.1.3.4 Dr. Serkan Aksoy
–
2009
5 These lecture notes are heavily based on the book of
Microwave Engineering
by David M. Pozar. For future versions or any proposals, please contact with
Dr. Serkan Aksoy
(saksoy@gyte.edu.tr).
3.
MICROWAVE NETWORKS
At low frequencies for electrically small circuits, lumped active and passive circuit elements are enough for analyzing the circuit leading a type of a Quasi-Static solution (assumption of negligible phase change in any where of the circuit) of Maxwell's equations and to Kirchoff Current and Voltage Laws with impedance concept. Moreover fields are considered as TEM type. But this way is not possible to analyze microwave circuits. The circuit concept should modify and apply to microwave network theory developed in MIT in 1940. The reasons of using it are as follow
Much easier than field theory, Calculations are performed at terminals, not everywhere, Easy to modify and combine different problems, The field solution of Maxwell's equation gives more information at the every time and place of the network, but difficult. At microwave frequencies, although the definition of the terminal pairs for line is relatively easy, the terminal pair for line does not strictly exist.
3.1.
Voltage, Current and Impedance
The measurements of and at microwave frequencies are difficult due to not easily defined terminals for non-TEM waves. Because of that the fields are measured and used as than, the impedance can be defined as . Because the fields depend on the coordinates (like in waveguide), special attenuation should be given for extraction of and . The way is to do that then, the impedance can be defined as. The impedance concept first used by O. Heaviside, and then after application to transmission lines, to electromagnetics by Schelkunoff. In this manner, types of it
Intrinsic Impedance, : It depends on only the material parameters. Wave Impedance, : TM, TE, TEM types are present which may depend on type of guide, material and frequency. Characteristic Impedance, : For TEM, it is unique, but for TE and TM, not unique because and can not be determined, uniquely.
It can be shown that the real parts of , and are even in , but the imaginery parts of them are odd in . and are the even function in .
3.2.
Impedance & Admittance Matrices
The and of a port microwave network having 'th terminal The impedance matrix is in the form of Similarly the admittance matrix is in the form of Clear that . It can be shown that Then and are known as
Input Impedance
and
Transfer Impedance
, respectively.
If the network is reciprocal (no ferrites, plasmas and active devices inside), and are the right relations. If the network is lossless, and are purely imaginary.
3.2.1.
Scattering Matrix
The form of the scattering matrix gives the
complete description of the port networks with the incident and reflected waves as Any element of the scattering matrix
Microwaves - Lecture Notes - v.1.3.4 Dr. Serkan Aksoy
–
2009
6 These lecture notes are heavily based on the book of
Microwave Engineering
by David M. Pozar. For future versions or any proposals, please contact with
Dr. Serkan Aksoy
(saksoy@gyte.edu.tr).
and are
Reflection
and
Transmission Coefficient
(from port to port ), respectively. Network analyzer is used to measure parameters of a network. If network is reciprocal, is symmetric. If network is lossless, is unitary means that. Using the relations as and with between and matrixes In the , all the and are defined as a reference point at the end of every lines. If the reference point is shifted, then where is the electrical length of the outward shift.
3.2.1.1.
Generalized Scattering Matrix
In the previous chapter, is defined for networks with same characteristic impedance for all ports. Generally for not same impedance for all ports, a new set of wave amplitudes as, Then, generalized matrix- In reciprocal networks, is symmetric,- In lossless networks, is unitary and satisfies the equation
3.2.2.
Transmission (ABCD) Matrix
Many microwave networks consisting cascade connection and need building block fashion in practice. ABCD matrix is defined to satisfy this as where port 1 and port 2 are completely isolated in the equation means that cascade multiplication is possible. The current direction is also specially designed for ABCD matrix. The relation between and matrix parameters are as If the network is reciprocal (), then .
3.3.
Equivalent Circuits for 2 Port Networks
Transition between a coaxial line and microstrip line can be chosen as an example of two port networks. Because of discontinuity in the transition region, EM energy is stored in the vicinity of the transition leading to reactive effects mean that the transition region should be modeled as black box (There is an unlimited way of equivalent circuits, but choosing matrix equivalence), then
A nonreciprocal network can not be represented by passive equivalent circuit using reciprocal elements. If the network is reciprocal (there are six degrees of freedom, six independent parameters), the presentations lead naturally to and equivalent circuits as If the network is lossless, the impedance and admittance matrix elements are purely imaginary, the degrees of freedom reduces to three and the elements of and equivalent circuits should be constructed from purely reactive elements.
3.4.
Signal Flow Graphs
Signal flow graph is an additional technique to analyse microwave networks in terms of reflected and transmitted waves. Three different forms of it are given below with nodes and branches.
Microwaves - Lecture Notes - v.1.3.4 Dr. Serkan Aksoy
–
2009
7 These lecture notes are heavily based on the book of
Microwave Engineering
by David M. Pozar. For future versions or any proposals, please contact with
Dr. Serkan Aksoy
(saksoy@gyte.edu.tr).
The decomposition rules are also given below
Microwaves - Lecture Notes - v.1.3.4 Dr. Serkan Aksoy
–
2009
8 These lecture notes are heavily based on the book of
Microwave Engineering
by David M. Pozar. For future versions or any proposals, please contact with
Dr. Serkan Aksoy
(saksoy@gyte.edu.tr).
4.
IMPEDANCE MATCHING
Impedance matching (or tuning) is an important issue for - Maximum power is delivered when load is matched to line(assuming the generator is matched)- Power loss is minimized.- ratio of receiver components is increased.- Amplitude and phase errors are reduced. Whenever has nonzero real part, impedance matching is possible with the factors such as- Complexity: Simpler one is prefable.- Wide Bandwidth: Match a load over a band.- Implementation: Easier one is prefable- Adjustability: Adjust to match a variable load impedance.
4.1.
L Networks Matching
The normalized should be converted to with adding impedance, then adding
–
the impedance matching will be successful.
4.2.
Quarter Wave Transformer
It is used for only real load impedance. Complex load impedance can always be transformed to real impedance by appropriate length of transmission line. But this generally alters the frequency dependency of the equivalent load reducing the bandwidth of the matching. The following relation has to be satisfied as where For multiple reflection, total is The condition of is also enough to make total reflection (multiple) is zero. If and , then and . For each frequency, has to be equal to . Thus fixed line length is possible only for one frequency. Bandwidth performance of QWT for wide band matching: If one set the maximum value of reflection coefficient, that can be tolerated, then the fractional bandwidth is This shows that as becomes closer to , the bandwidth increases. This result is valid only for TEM lines. The step changes of reactance effect can be compensated by making a small adjustment in the length of the matching section. Approximate behavior of reflection coefficients is shown at below. The QWT can be extended as a multisection form for matching of broader bandwidth.
4.3.
Single Stub Tuning
A single open-circuited (or short-circuited) transmission line is connected either in parallel or series with the feed line at a certain distance from the load. Single Sub Tuning can match any load impedance to line, but suffer from disadvantage of requiring a variable length between the load and stub.
Microwaves - Lecture Notes - v.1.3.4 Dr. Serkan Aksoy
–
2009
9 These lecture notes are heavily based on the book of
Microwave Engineering
by David M. Pozar. For future versions or any proposals, please contact with
Dr. Serkan Aksoy
(saksoy@gyte.edu.tr).
Since lumped elements are not required, single stub is convenient and easy to fabricate in microstrip form. Two adjustable parameters and susceptance or reactance provided by stub. Although for microstrip lines open circuit is easy to fabricate since a via-hole is enough, for coax or waveguide short circuit is preferred since open circuit line may be large for radiation. If the impedance has the form of at the distance . Then stub reactance can be chosen as
–
, resulting for matching condition. For a given susceptance or reactance, the difference in lengths of open and short-circuited stub is .
4.4.
Double Stub Tuning
The double stub tuner can not match all load impedances, but load may be arbitrary distance from the first stub. Distance between the stubs should be generally chosen as or to reduce the frequency sensitivity.
Single Section Transformer
: The reflection coefficient of single section transformer can be written when discontinuities between the impedances are small as This shows that is dominated by and .
Multisection Transformer
: If the applications require more bandwidth, multisection transformers consists of equal length sections of the lines can be used. The reflection coefficient can be written as The importance of this result is that the desired reflection coefficients response as a function of frequency can be synthesized by proper choosing of . To obtain passband responses, binominal (maximally flat) and Chebysev (equal ripple) multisection matching transformers can be used. In first one: the derivatives of is settled to zero, in second one: is equated to Chebyshev polynomial.
4.5.
Tapered Lines
The line can be continuously tapered for decreasing the effect of the step changes in characteristic impedance between the discrete sections. The incremental reflection coefficient Since , by using theory of small reflections where from can be found. Chancing type of taper (Exponential, , Triangular, Klopfenstein), different band pass characteristic may be applied. Klopfenstein yields the shortest matching section. The Bode-Fano criterion for certain type of canonical load impedances will help us to define theoretical limit on the minimum reflection with the upper limit of matching performance and provide a benchmark against which a practical design can be compared.
Microwaves - Lecture Notes - v.1.3.4 Dr. Serkan Aksoy
–
2009
10 These lecture notes are heavily based on the book of
Microwave Engineering
by David M. Pozar. For future versions or any proposals, please contact with
Dr. Serkan Aksoy
(saksoy@gyte.edu.tr).
5.
POWER DIVIDERS & COUPLERS
These are passive components used for power division or power combining. In power division, an input signal is divided by coupler in two (or more) signals, equally or not.
5.1.
Three Port Networks (T Junction)
It has two inputs with one output.
If component is passive (no anisotropic material), the network is reciprocal and when all ports are also matched, considering lossless one Using the features of for lossless and reciprocal network To satisfy, above equation at least two parameters have to be zero means that three port network can not be reciprocal, lossless and matched all ports. If the network is nonreciprocal with matching all port and satisfaction of energy conservation, such a device is known as
Circulator
relies on anisotropic materials. if only two ports of the network are matched, a lossless and reciprocal network can be physically realizable. If the network is being lossy, network can be reciprocal and matched at all ports (
Resistive Divider
or
Isolator
). As an example,
Ferrite Isolators
are two-port device having unidirectional transmission characteristics. Because is not unitary, the isolator must be lossy. The isolators can be used between a high-power source and load to prevent possible reflections from damaging the source by absorbing reflected power.
5.1.1.
T Junction Power Divider
This can be used for power division (or combining).
Lossless Divider
: This suffers from the problem of not being matched at all ports and in addition does not have any isolation between two output ports. The fringing fields and higher order modes at the discontinuity leading stored energy can be accounted by a lumped susceptance, . The output line impedances and can be selected to provide various power decision.
Resistive Divider
: Possible to match all ports simultaneously, the resistive (lossy) divider is used, but no isolation between two output ports due to being not lossless. Half of the supplied power is dissipated in resistors.
5.2.
Four Port Networks (Directional Coupler)
It has two inputs and two outputs. After considering using the features of matrix for reciprocal, matched and lossless network, the possible solutions are means
Directional Coupler
. Using different phase references,
Symmetrical
or
Anti-symmetrical
Directional Coupler
may be defined. The design parameters of directional coupler are The coupling factor shows the fraction of input power to the output. The directivity is a measure of isolation ability for forward and backward waves. The ideal coupler has infinite directivity and isolation and also lossless. The directional property of the all directional coupler is produced through the use of two separate waves or wave components, which add in phase at the coupled port, and cancel in phase at the isolated port.
5.2.1.
Waveguide Directional Coupler
Bethe Hole Coupler
: Couple one waveguide to another through a single small hole in the common wall. Types of the parallel guides and skewed guides work properly only at the design frequency (narrow bandwidth in terms of its directivity).
Multi Hole Coupler
: Series of coupling holes are used to increase bandwidth as similar design to multi section transformer. Making coupling coefficients proportional to binominal coefficients, maximally flat response can be obtained. Using Chebysev polynomial, different responses are possible.
Microwaves - Lecture Notes - v.1.3.4 Dr. Serkan Aksoy
–
2009
11 These lecture notes are heavily based on the book of
Microwave Engineering
by David M. Pozar. For future versions or any proposals, please contact with
Dr. Serkan Aksoy
(saksoy@gyte.edu.tr).
5.2.2.
Wilkinson Power Divider
It is a network with the useful property of being lossless when the output ports are matched, that is, only reflected power is dissipated. It is known that a lossy three port network can be made having all ports are matched with isolation between the output ports. Wilkinson Power Divider can be made in microstrip or stripline form with arbitrary power division of way Divider or Combiner. The even-odd mode technique is used for analysis.
5.2.3.
Hybrid Coupler
It has having types of the following.
5.2.3.1.
Quadrature Hybrid ( Hybrid)
This is a directional coupler (knows as
Branch Line Hybrid
) with a phase difference in outputs (2 3). Even- odd mode technique can be applied for analysis. matrix has a high degree of symmetry means any port can be used for input as given below
5.2.4.
Hybrid
It is a four port network with a phase shift (2 3) between two outputs (also may be in phase). It can be used as a combiner and has unitary symmetric scattering matrix as It may be produces as the form of ring hybrid (rate race), tapered matching lines and hybrid waveguide junction (Magic T, (Rate Race)) in which symmetrically (or antisymmetrical) placed tuning ports (or irises) can be used for matching.
5.2.5.
Coupled Line Directional Coupler
Coupled lines of two (or more) transmission lines are closed together, power can be coupled between the lines. Generally TEM mode is assumed rigorously valid for striplines, but approximately valid for microstrips. Coupled Line Theory is based on types of excitations as even mode (strip currents are equal in amplitude with same directions) and odd mode (strip currents are equal in amplitude with opposite directions). Arbitrary excitation can be treated as a superposition of appropriate even and odd modes amplitudes. Moreover design graphs are present for coupled lines.
Design Considerations:
- Although a single section coupled line has limited bandwidth due to requirement, the bandwidth can be increased using multiple sections coupled line having close relations to multisection QWT.- The assumption of the same velocity of propagation for even and odd modes in design, generally not satisfied for a coupled microstrip or non TEM lines. This gives poor directivity. By using more effective dielectric constant (smaller phase velocity) for even mode, phase differences should be minimized. This also produces problems as the mismatching phase velocities for multisection case and degrades coupler directivity. Increasing bandwidth can be obtained with low coupling limits.
5.2.6.
Lange Coupler
To increase coupling factor, Lange Coupler (several lines) with phase difference between outputs is used as a 3 dB coupling ratio in an octave or more bandwidth can be achieved. The main disadvantage of it(a type of quadrature hybrid) is difficult to fabricate due to very narrow lines. Folded Lange coupler is also used for more easily analysis to model equivalent circuit.
5.3.
Other Couplers
Moreno Crossed Guide Coupler
Schwinger Reversed Phase Coupler
Riblet Short Slot Coupler
Symmetric Tapered Coupled Line Coupler
Coupler with Apertures in Planar Lines
As an example of a device uses a directional coupler is
Reflectometer
isolate and sample the incident and reflected powers from a mismatch load as a heart of a scalar (or vectorial) network analyzer.
Microwaves - Lecture Notes - v.1.3.4 Dr. Serkan Aksoy
–
2009
13 These lecture notes are heavily based on the book of
Microwave Engineering
by David M. Pozar. For future versions or any proposals, please contact with
Dr. Serkan Aksoy
(saksoy@gyte.edu.tr).
If the line is at the temperature , .
Noise Figure of Cascaded System
: A cascaded system of two components (), () and The output of first stage : The output of second stage: where and . The first stage is dominant due to reduces to second stage. Generally
Noise Figure of a Passive Two Port Network
:
Available Power Gain
does not depend on . where , then is as The definitions of and are close as lossy lines. When the network is matched , then
Noise Figure of a Mismatched Lossy Line
: Previously, Noise Figure of a lossy line is calculated under assumptions of line is matched to its input and output circuits. Consider that line is mismatched to input circuit as Then When the line is matched same as the matched lossy line.
6.2.
Dynamic Range & Intermodulation Distortion
All realistic devices are nonlinear at very low power levels due to noise effects and also practical components became nonlinear at high power levels. A given component (or network) can operate as desired between minimum and maximum realistic power ranges known as
Dynamic Range
. In the sense of intermodulation distortion, it is called as
Spurious Free Dynamic Range
. The output response of a nonlinear device(diode, transistor) by using a Taylor series expansion where is DC output, is Lineer output, others are Nonlinear outputs. Different output response can be obtained relating to coefficients as Only , Rectifier Only , Attenuator or Amplifier Only , Mixing or Frequency Conversion
Gain Compression:
In most practical system, , then gain tends to decrease named
Gain Compression
or
Saturation
.
Intermodulation Distortion:
2
the output is the combination of two input frequencies are called
Intermodulation Products
. Passive Intermodulation: Connectors, cables, antennas, and every metal-metal contact can cause passive intermodulation due to poor mechanical contact, oxidation, contamination etc., and also thermal effects of high power source. This has generally lower power levels.
Microwaves - Lecture Notes - v.1.3.4 Dr. Serkan Aksoy
–
2009
14 These lecture notes are heavily based on the book of
Microwave Engineering
by David M. Pozar. For future versions or any proposals, please contact with
Dr. Serkan Aksoy
(saksoy@gyte.edu.tr).
6.3.
RF Diode Characteristics
Shottky Barrier Diode Detectors
: This is a nonlinear device consisting of semiconductor-metal junction resulting lower junction capacitance can be used frequency conversion(rectification, detection, mixing). It has a with a Small Signal Model These diodes are used as rectifiers, detectors and demodulation of an AM modulated RF carrier.
PIN Diode:
This is used to construct an electronic switching for control circuits such as phase shifters and attenuators. These are preferable because of small size, high speed and inerrability with planar circuits. Especially single-pole PIN diode switches can be used in either a series or a shunt configuration to form a single pole RF switch. Insertion Loss of switches where is diode impedance as
Varactor Diode
: Junction capacitance varies with bias voltage used for electronically frequency tuning.
Impatt Diode
: Similar to PIN diode, but based on avalanche effects exhibiting negative resistance over a broad frequency range, therefore used to directly convert DC to RF power.
Gunn Diode
: It exhibits a negative differential resistance based on Gunn effect and used to generate RF power to DC.
Baritt Diode
: Similar to junction transistor without a base contact and useful for detector and mixer applications with advantages of lower AM noise.
Microwaves - Lecture Notes - v.1.3.4 Dr. Serkan Aksoy
–
2009
16 These lecture notes are heavily based on the book of
Microwave Engineering
by David M. Pozar. For future versions or any proposals, please contact with
Dr. Serkan Aksoy
(saksoy@gyte.edu.tr).
If device is unconditionally stable, the stability circles must be completely outside (or totally enclose) the Smith chart. This can be stated mathematically as for for If or , the amplifier can not be unconditionally stable because a source (or load impedance) leading to (or ) can cause (or ). If transistor is only conditionally stable, and must be chosen in stable regions. Specially unconditionally stability can be tested with the methods of
Rollet’s Condition
or
Parameter
.
7.3.
Single Stage Amplifier Design
Maximum gain with stability can be realized when input and output sections provide a conjugate match between source and load impedance, but generally as a narrowband. To perform this conditions simultaneously have to be satisfied means that also by maximizing the transducer gain, first of all , then should be solved by considering stability conditions. It is also preferable to design for less than the maximum obtainable gain, to improve bandwidth (or to obtain a specific amplifier gain). To do that,
Constant Gain Circles
on the Smith chart to represent loci of and that give fixed values of gain are used. Besides stability and gain, the Noise Figure of the amplifier should be minimized by using
Constant Noise Figure Circles
.
7.4.
Broadband Amplifier Design
The bandwidth can be improved with designing for less than maximum gain will improve bandwidth, but the input and output ports will be poorly matched. Common approaches to solve this problem are listed below-
Compensated Matching Network,-
Resistive Matching Network,-
Negative Feedback,-
Balanced Amplifiers,-
Distributed Amplifiers.
7.5.
Power Amplifiers
This is used to increase power level with consideration of efficiency, gain, intermodulation and thermal effect.
Amplifier Efficiency
is defined as with the effect of input power,
Power Added Efficiency, PAE
where is power gain.
PAE
drops quickly with frequency. Another parameter is
Compressed Gain
defined as the gain of amplifier at 1 dB compression gain as where is small signal (linear) power gain. Class A amplifiers with theoretically maximum efficiency are inherently linear that transistor is biased to conduct over entire range of input signal cycle (low-noise amplifier). Class B amplifiers with theoretically maximum efficiency are biased to conduct only during one-half of input signal cycle (Push-Pull amplifier). Class C amplifiers with efficiency near are operated with transistor near cut-off for more than half of the input signal cycle (in a resonant circuit, constant envelope modulation). Higher classes such as D, E, F and S are also used with high efficiency.
7.5.1.
Large Signal Characterization
If input power is small enough, parameter is independent from input power and linear small signal model is suitable for modeling. But for high input powers, transistor behaves as a nonlinear device (
Large-Signal Characterization
) and more difficult to design. The following methods are possible for Large Signal Characterization-
Measure the output power as a function of source and load impedances and produce tables, then determine large signal source and load reflection coefficients to maximize power gain for a particular output power.-
Plot contours(
Load-Pull Contours
) of constant power output on a Smith chart as a function of load reflection coefficient with conjugately matching at input and design for a specified gain.-
Use nonlinear equivalent of the transistor circuit. Especially for designing Class A amplifiers, the stability can be checked by using small signal model because instabilities begin at low signal levels.

# Lecture Notes - Microwaves

Download this Document for FreePrintMobileCollectionsReport Document

#### Report this document?

Please tell us reason(s) for reporting this document

Spam or junk

Porn adult content

Hateful or offensive

If you are the copyright owner of this document and want to report it, please follow these directions to submit a copyright infringement notice.

Cancel

This is a private document.

### Info and Rating

Reads:
10
Uploaded:
04/20/2011
Category:
Uncategorized.
Rated:
Copyright:
Attribution Non-commercial

Follow
Paspulati Leelaram

### Share & Embed

### More from this user

PreviousNext

1. 18 p.
   17 p.

### Add a Comment

Characters: 400

### Print this document

### High Quality

Open the downloaded document, and select print from the file menu (PDF reader required).

### Sign up

Use your Facebook login and see what your friends are reading and sharing.

#### Other login options

Login with Facebook

### Signup

I don't have a Facebook account

email address (required)
create username (required)
password (required)

| Send me the Scribd Newsletter, and occasional account related communications.

Privacy policy
You will receive email notifications regarding your account activity. You can manage these notifications in your account settings. We promise to respect your privacy.

### Why Sign up?

| Discover and connect with people of similar interests.
| Publish your documents quickly and easily.
| Share your reading interests on Scribd and social sites.

Already have a Scribd account?

email address or username
password
Trouble logging in?

### Login Successful

Now bringing you back...

« Back to Login

### Reset your password

Please enter your email address below to reset your password. We will send you an email with instructions on how to continue.

Email address: |
You need to provide a login for this account as well.
Login: |

scribd. scribd. scribd. scribd. scribd. scribd. scribd. scribd. scribd. scribd. scribd. scribd. scribd. scribd. scribd. scribd. scribd.